[HEADER]
VERSION=10

[_EXTENSION]
EXTENDED_RAYTRACING=1

[VIRTUALKM]
USE_LOAD=1

[COMPOUND_DEFAULT]
INDEX=0

[__CM_FRONT_ORIGINAL]
NAME=Potenza RE070
SHORT_NAME=ST
WIDTH=0.225
RADIUS=0.3185
RIM_RADIUS=0.254
ANGULAR_INERTIA=1.6507
DAMP=500
RATE=298926
DY0=1.3053
DY1=-0.048
DX0=1.3142
DX1=-0.046
WEAR_CURVE=t_wear_curve_RE070.lut
SPEED_SENSITIVITY=0.003470
RELAXATION_LENGTH=0.07200
ROLLING_RESISTANCE_0=12
ROLLING_RESISTANCE_1=0.001023
ROLLING_RESISTANCE_SLIP=5011
FLEX=0.000686
CAMBER_GAIN=0.115
DCAMBER_0=1.2
DCAMBER_1=-13
FRICTION_LIMIT_ANGLE=7.52
XMU=0.27
PRESSURE_STATIC=29
PRESSURE_SPRING_GAIN=8890
PRESSURE_FLEX_GAIN=0.4
PRESSURE_RR_GAIN=0.55
PRESSURE_D_GAIN=0.0045
PRESSURE_IDEAL=37
FZ0=2939
LS_EXPY=0.8174
LS_EXPX=0.8756
DX_REF=1.30
DY_REF=1.28
FLEX_GAIN=0.0302
FALLOFF_LEVEL=0.86
FALLOFF_SPEED=2
CX_MULT=1.04
RADIUS_ANGULAR_K=0.01
BRAKE_DX_MOD=0.05

[__CM_THERMAL_FRONT_ORIGINAL]
SURFACE_TRANSFER=0.0140
PATCH_TRANSFER=0.00027
CORE_TRANSFER=0.00057
INTERNAL_CORE_TRANSFER=0.0052
FRICTION_K=0.05184
ROLLING_K=0.22
SURFACE_ROLLING_K=1.42024
PERFORMANCE_CURVE=t_temp_curve_RE070.lut
GRAIN_GAMMA=1
GRAIN_GAIN=0.4
BLISTER_GAMMA=1
BLISTER_GAIN=0.4
COOL_FACTOR=2.73

[__CM_REAR_ORIGINAL]
NAME=Potenza RE070
SHORT_NAME=ST
WIDTH=0.225
RADIUS=0.3185
RIM_RADIUS=0.254
ANGULAR_INERTIA=1.6105
DAMP=500
RATE=298926
DY0=1.3053
DY1=-0.048
DX0=1.3142
DX1=-0.046
WEAR_CURVE=t_wear_curve_RE070.lut
SPEED_SENSITIVITY=0.003470
RELAXATION_LENGTH=0.07200
ROLLING_RESISTANCE_0=12
ROLLING_RESISTANCE_1=0.001023
ROLLING_RESISTANCE_SLIP=5011
FLEX=0.000686
CAMBER_GAIN=0.115
DCAMBER_0=1.2
DCAMBER_1=-13
FRICTION_LIMIT_ANGLE=7.52
XMU=0.27
PRESSURE_STATIC=29
PRESSURE_SPRING_GAIN=8890
PRESSURE_FLEX_GAIN=0.4
PRESSURE_RR_GAIN=0.55
PRESSURE_D_GAIN=0.0045
PRESSURE_IDEAL=37
FZ0=2939
LS_EXPY=0.8174
LS_EXPX=0.8756
DX_REF=1.30
DY_REF=1.28
FLEX_GAIN=0.0302
FALLOFF_LEVEL=0.86
FALLOFF_SPEED=2
CX_MULT=1.04
RADIUS_ANGULAR_K=0.01
BRAKE_DX_MOD=0.05

[__CM_THERMAL_REAR_ORIGINAL]
SURFACE_TRANSFER=0.0140
PATCH_TRANSFER=0.00027
CORE_TRANSFER=0.00057
INTERNAL_CORE_TRANSFER=0.0052
FRICTION_K=0.05184
ROLLING_K=0.22
SURFACE_ROLLING_K=1.42024
PERFORMANCE_CURVE=t_temp_curve_RE070.lut
GRAIN_GAMMA=1
GRAIN_GAIN=0.4
BLISTER_GAMMA=1
BLISTER_GAIN=0.4
COOL_FACTOR=2.73

[REAR]
NAME=Semislicks
SHORT_NAME=SM
WIDTH=0.2150
RADIUS=0.31260
RIM_RADIUS=0.2286
ANGULAR_INERTIA=1.3100
DAMP=500
RATE=254719
DY0=1.2873
DY1=-0.0480
DX0=1.2968
DX1=-0.0460
WEAR_CURVE=__cm_tyre_wearcurve_rear_0.lut
SPEED_SENSITIVITY=0.003490
RELAXATION_LENGTH=0.07253
ROLLING_RESISTANCE_0=12
ROLLING_RESISTANCE_1=0.0010300
ROLLING_RESISTANCE_SLIP=4970
FLEX=0.00069200
CAMBER_GAIN=0.136
DCAMBER_0=1.20
DCAMBER_1=-13
FRICTION_LIMIT_ANGLE=7.99
XMU=0.27
PRESSURE_STATIC=26
PRESSURE_SPRING_GAIN=7874
PRESSURE_FLEX_GAIN=0.40
PRESSURE_RR_GAIN=0.55
PRESSURE_D_GAIN=0.0045
PRESSURE_IDEAL=31
FZ0=2494
LS_EXPY=0.8119
LS_EXPX=0.8791
DX_REF=1.300
DY_REF=1.280
FLEX_GAIN=0.0304
FALLOFF_LEVEL=0.86
FALLOFF_SPEED=2
CX_MULT=1.04
RADIUS_ANGULAR_K=0.0100
BRAKE_DX_MOD=0.05
__CM_SOURCE_ID=ktm_xbow_r

[THERMAL_REAR]
SURFACE_TRANSFER=0.0165
PATCH_TRANSFER=0.00027
CORE_TRANSFER=0.0001400
INTERNAL_CORE_TRANSFER=0.003800
FRICTION_K=0.07719
ROLLING_K=0.22
PERFORMANCE_CURVE=__cm_tyre_perfcurve_rear_0.lut
GRAIN_GAMMA=1.0000
GRAIN_GAIN=0.40
BLISTER_GAMMA=1.0000
BLISTER_GAIN=0.4
COOL_FACTOR=1.88
SURFACE_ROLLING_K=1.25049

[FRONT]
NAME=Semislicks
SHORT_NAME=SM
WIDTH=0.2150
RADIUS=0.31260
RIM_RADIUS=0.2286
ANGULAR_INERTIA=1.3100
DAMP=500
RATE=254719
DY0=1.2873
DY1=-0.0480
DX0=1.2968
DX1=-0.0460
WEAR_CURVE=__cm_tyre_wearcurve_front_0.lut
SPEED_SENSITIVITY=0.003490
RELAXATION_LENGTH=0.07253
ROLLING_RESISTANCE_0=12
ROLLING_RESISTANCE_1=0.0010300
ROLLING_RESISTANCE_SLIP=4970
FLEX=0.00069200
CAMBER_GAIN=0.136
DCAMBER_0=1.20
DCAMBER_1=-13
FRICTION_LIMIT_ANGLE=7.99
XMU=0.27
PRESSURE_STATIC=26
PRESSURE_SPRING_GAIN=7874
PRESSURE_FLEX_GAIN=0.40
PRESSURE_RR_GAIN=0.55
PRESSURE_D_GAIN=0.0045
PRESSURE_IDEAL=31
FZ0=2494
LS_EXPY=0.8119
LS_EXPX=0.8791
DX_REF=1.300
DY_REF=1.280
FLEX_GAIN=0.0304
FALLOFF_LEVEL=0.86
FALLOFF_SPEED=2
CX_MULT=1.04
RADIUS_ANGULAR_K=0.0100
BRAKE_DX_MOD=0.05
__CM_SOURCE_ID=ktm_xbow_r

[THERMAL_FRONT]
SURFACE_TRANSFER=0.0165
PATCH_TRANSFER=0.00027
CORE_TRANSFER=0.0001400
INTERNAL_CORE_TRANSFER=0.003800
FRICTION_K=0.07719
ROLLING_K=0.22
PERFORMANCE_CURVE=__cm_tyre_perfcurve_front_0.lut
GRAIN_GAMMA=1.0000
GRAIN_GAIN=0.40
BLISTER_GAMMA=1.0000
BLISTER_GAIN=0.4
COOL_FACTOR=1.88
SURFACE_ROLLING_K=1.25049

